**Improvement of Solar PV Unit Competence through Neem oil as Coolant**

**M. Saravanapandian1, S. Athimoolam2, L. Manoharan3, S. Sivakumar4**

1, 2 Department of ECE, PSR Engineering College, Sevalpatti, Sivakasi, Virudhunagar, India, 3 Department of ECE, Hindustan Institute of Technology and Science, Padur, Chennai, India, 4 Department of ECE, Bharat Institute of Higher Education and Research, Selaiyur,Chennai,India.

[*saravanapandian@psr.edu.in*](mailto:saravanapandian@psr.edu.in)1, [*athimoolam@psr.edu.in*](mailto:athimoolam@psr.edu.in)2, [*manoharanekk@gmail.com3*](mailto:manoharanekk@gmail.com3)*,* [*sivacud@gmail.com*](mailto:sivacud@gmail.com) *4*

**Abstract**

The Solar PV cells are used to convert the sunlight into electricity and Sunlight radiation also have heat which is reduced to efficiency of the panel. The heat should be controlling the limited value or otherwise reduced the performance of the panel so that, heat is move to the cooling medium thus maintaining the heat in functioning limit. The proposed method is explained in the probability of cooling the monocrystalline and polycrystalline structure is used as neem oil through incorporated oil container fitted into backside of the unit. The neem oil is not polluted the environment, thus also used to exchange noxious mineral oil. The neem oil moved from depository tank to backside of the unit and together in an additional depositor tank, thus be able to reuse. The proposed method is detailed investigated and functioning comparison takes place different PV type such as monocrystalline and polycrystalline module with various kind of edible oil. Thus, the important outcomes of method are decrease the panel temperature and enhance efficiency of the PV panel. The viscosity and calorific value are important parameter of cooling oil.

**Keywords:** Solar PV, Waste Neem Oil, Cooling, Efficiency.

**1. Introduction**

The occurrence sunlight of able to be seen wavelength upper limit is 1200nm and lower limit is 400nm are immersed with the solar panel and transformed into electrical energy. The occurrence solar light also has a heat this increases the panel temperature. The real time competence of the monocrystalline unit is 12-18%, respected to the lab competence of 25% [1, 2]. In ref, [3], the novelist experiential so as to the standard competence have monocrystalline & polycrystalline unit throughout summer reductions through 20.1% & 19.6%, compared to wintertime.

The burning dry area, the functioning heat as PV be able toward amplify up to 81°C [4] but in the steamy area, amplify further than the functioning limits, thus give on to thermal deprivation and decrease in competence [5]. The deprivation in the exchange competence of 0.51% reduces occurs for each 0.9°C increase [6, 7]. In adding together, to amplify in functioning heat, partial shading and hot-spot influence the competence [8-13]. In a series connection cells have partial shading; thus, cell operate to the load so that losses the power as heat. Thus, kind of problem is overcome by connecting bypass diode transversely to series linked cells [9, 14]. The warm-plug decreases on competence& produce warm air pressure happening as compartment thus dropping on consistency of the arrangement [9]. Consequently, the situation is very important toward remove temperature as of the PV cell. The temperature generates in the unit be able to decreased by means of wind or liquid by way of a cooling materials as rear on frontage exterior.

In wind-cooled solar arrangements are cast-off on different and economical resolution to construction an incorporated arrangement. The wind hole connecting the unit and rooftop is able to use for circulate the wind to reduce the temperature of PV unit and preheated wind be able to use for construction thermal needs. [15, 16] To analysis the construction-incorporated PV arrangement and used the usual wind to reduce the temperature of the unit. The wind run is determined by the temperature and wind-produced force among the apex and base of the space. Likewise, numerous methods such as fins [17], matrix [18], and crowded wind flow way [19] has used as cooling medium of the PV unit.

In Ref [20] considered the process of dropping the indication on the PV unit by means of a layer (0.9 mm) of operation water on the frontage exterior of the unit. The outcomes how amplify in functioning of 10.6% in excess of the day. In Ref [21] investigated the functioning of the PV arrangement by give water on the higher exterior of the unit. The investigated confirmation is to amplify of 16% in the competence at tip emission circumstances. In Ref [22] better-quality the functioning on solar water drive arrangement with scattering water in excess on frontage exterior of the unit. The novelist establishes so as to the spraying aquatic to the frontage exterior decreases the indication and heat of the PV panel. In Ref [23] analysis the functions of the unit flooded in water and improved the competence of the arrangement.

Together wind and water are able to use as a cooling intermediate to move the temperature generate by the unit. On the other hand, the PV arrangement by means of water as a cooling intermediate is additional competent as compared with air owing towards its high value thermo substantial belongings. [24].

The mineral oil is used as a cooling intermediate for the move to produce noxious matter owing toward oxidative unsteadiness. The method of tools breaks down; the removal of inorganic oils remains hard. The out flow of inorganic oils be able to reason a severe hazard to the atmosphere. Consequently, silicon oil is used as another to mineral oil contain a high value flash factor; it is additional costly and not well for environment. Hence, vegetable oil be able used as an exchange cooling intermediate for transferable, thus is obtainable highly, inexpensive, renewable, recyclable and safe one. Vegetable oil is triglyceride extract as of vegetation or the seed and turn out to be fluid at room hot ness [25].

In this examine, this inspection be used waste edible oil such as peanut oil cast-off as the temperature transport liquid to uphold on necessary functioning heat of the unit. The edible oil has benefitted concentration owing towards its accessibility, reuse environment friendly, less hazards and small influence happening the atmosphere [26]. Vegetable has enhanced thickness, flash factor, dielectric power and secure flames better to mineral exchange oils (peanut oil) intimated in Table 1. Depends happening the final use of vegetable oils are intimated as edible oil.

The arrangement of the manuscript is prepared as addressed part 2 explains the investigational setup designed for solar PV scheme lacking and by means of the cooling preparation. Part 3 explains the outcome and talk for investigational examination of peanut oil as temperature move fluid beside through a conclusion in part 4.

**2. Investigational setup**



**Figure 1.** Representation diagram of the proposed system



**Figure 2. (a)** Solar unit with a cooling preparation **(b)** Rear lubricant tank

Figure. 1 shows the representation diagram of the proposed system. The construction of solar unit, waste oil depositary tank, rear oil tank incorporated through PV unit, force air drive, and oil tank for bring together waste oil. The functioning on solar unit by way of a purpose of eatable oil cooling bean investigation with via a monocrystalline and polycrystalline unit (17-inch × 14-inch) not including and including cooling part beside through rear agreement oil depositary tank of 16 inch × 13 inch × 1.6. The investigational setup (Figure 2) is designed at the rooftop of the KCET (9.6728° N, 77.9659° E). The occurrence sunlight and heat of the PV unit are calculated with the solar indicator. Together the unit construct of oil-incorporated tank fitted towards the rear of PV unit for interesting the temperature as of the unit and thus uphold the necessary functioning heat. The waste edible oil (peanut lubricant) remains deposit to depositary tank; the situation is approved to run from end to end the oil tank part inside the rear on PV unit. In regulator wheel the oil run keen on the unit in addition to away of the unit. Thus, excited oil is together on depositary tank. The functioning investigation on monocrystalline and polycrystalline unit not including in addition to including oil cooling actions is behaviour through edible oil similar to peanut oil (05.04.2020) since coolant.

**Table 1** Substantial belongings of edible oil [27, 28]

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Requirement** | **Thickness (g/ml)** | **Kinematic Viscosity @40 °C (mm2/sec)** | **Thickness Index** | **Saponification Value** | **Iodine Value** | **Pour Factor °C** | **Flash Factor °C** |
| Peanut oil | 0.914 | 36.84 | 144 | 184-195 | 84-95 | 3 | 336 |

**3. Results Analysis**

3.1 Peanut oil

The highest sunlight of 940W/m2is inward at 01.00 P.M, lowest amount sunlight of 80W/m2is inward at 6.00 P.M and standard sunlight inward all the way through the daylight (05.04.2022) is 633 W/m2. The highest ambient heat is 41.4oC evidence at 01.00 P.M, least amount ambient heat is 26.4oC establish at 09.00 A.M and standard heat throughout the daylight is 32.83oC (Table 2).

Figure. 3 intimates the force of peanut oil cooling lying on unit heat all the way through the daylight. The highest, smallest amount and standard unit heat for the monocrystalline unit not including cooling is 68.5oC, 30.3oC and 51.3oC and including cooling, is 66.3oC, 28oCand 49.19oC correspondingly. The peanut oil since the coolant has outcome with in a standard decrease of the monocrystalline unit and polycrystalline unit heat as2.29% and 04.34% correspondingly.

**Figure 3.** Unit temperature for peanut oil as a coolant through time

Figure. 4 intimates on difference of sunlight with respect to time. The greatest and smallest amount sunlight occurs on 01.00 P.M and 06.00 P.M. The unit heat amplify with amplify in sunlight.

**Figure 4.** Solar irradiation for peanut oil as a coolant through time

In highest, value of competence for monocrystalline unit not including and including cooling is 11.6% and 12.8% experiential at 10.00 A.M. likewise for polycrystalline unit not including and including cooling is 12.9% experiential at 10.00 A.M and 19.8% at 6.00P.M. Consequently, the monocrystalline and polycrystalline unit contain improved the standard competence towards15.0% and 17.8% through the cooling unit.

**Figure 5.** Output power for not including cooling unit through time

**Figure 6.** Output power for including (Peanut oil as a coolant)

cooling unit through time

**Table 2** Peanut oil as a coolant

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Time** | **Solar irradiation** | **Ambient temperature** | **Monocrystalline unit not including cooling arrangement** | | **Polycrystalline unit not including cooling arrangement** | | **Monocrystalline unit including cooling arrangement** | | **Polycrystalline unit including cooling arrangement** | | |
| **Module temperature** | **Output power** | **Module temperature** | **Output power** | **Module temperature** | **Output power** | | **Module temperature** | **Output power** | |
| 9 | 400 | 26.4 | 30.3 | 19.1 | 29.9 | 22.1 | 28 | 21.1 | | 27 | 25 | |
| 10 | 710 | 30.3 | 50.2 | 29.2 | 49.1 | 31.2 | 48.3 | 31.3 | | 47.2 | 34.3 | |
| 11 | 890 | 33.7 | 57.2 | 37.1 | 56.9 | 38.9 | 55.1 | 39.3 | | 54.9 | 40.9 | |
| 12 | 910 | 38.4 | 64.2 | 36.2 | 63.1 | 38.6 | 62.8 | 38.4 | | 61.2 | 40.4 | |
| 13 | 940 | 41.4 | 68.5 | 37.3 | 67.1 | 39.4 | 66.3 | 39.9 | | 65.2 | 41.6 | |
| 14 | 860 | 35.6 | 56.7 | 34.2 | 55.1 | 37 | 54.7 | 36.2 | | 53 | 39.8 | |
| 15 | 700 | 34.2 | 56.3 | 26.6 | 55.2 | 28.9 | 54.2 | 28.7 | | 53.1 | 30.9 | |
| 16 | 520 | 32 | 51.1 | 19.6 | 50.3 | 22 | 49 | 21.7 | | 48.2 | 24.6 | |
| 17 | 320 | 29.6 | 42.7 | 11.4 | 41.2 | 14 | 40.2 | 13.6 | | 39.1 | 16.3 | |
| 18 | 80 | 26.7 | 35.8 | 1 | 34.1 | 4 | 33.3 | 2.2 | | 32 | 5.1 | |

**4. Summarize of functioning on peanut oil as a coolant**

**Table 3** Evaluation of PV unit through cooling Construction

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Edible oil** | **Decrease in unit temperature for the monocrystalline unit including cooling** | **Decrease in unit temperature for the polycrystalline unit including cooling** | **Enhancement in competence for the monocrystalline unit including cooling** | **Enhancement in competence for the polycrystalline unit including cooling** |
| **Peanut oil** | 2.29% | 4.34% | 15.0% | 17.80% |

Table 3 signify the evaluation of decrease in unit heat and enhancement in competence for not including and including cooling intended in favour of the monocrystalline and polycrystalline unit. Beginning the Table, it is concluded so as to the polycrystalline unit have enhanced the functioning on unit beneath the complete cooling intermediate. Designed for everyone, the polycrystalline unit function improved than the monocrystalline unit. The monocrystalline and polycrystalline unit functioning beneath peanut oil since the cooling intermediate has created better functioning.

**Conclusion**

The work evaluated the possibility of rear exterior cooling of the monocrystalline and polycrystalline unit with means of waste edible oil as coolant. At this time, the ecological gracious edible is use as an exchange towards the mineral oil. The function of the unit including and not including coolant is experiential for dissimilar edible oil similar to peanut oil. The peanut oils, the competence of the monocrystalline and polycrystalline unit amplifies towards 15.0% and 17.80%. Beginning the experiential outcome, the work proposes so as to the waste edible oil be able to use as coolant exchange towards the noxious mineral oil or water in container of shortage. The use edible oil since a coolant is a cost reduction, atmosphere gracious, which be able to incorporated keen on the unit to uphold the necessary functioning heat. In opportunity, the build-up temperature in oil be able to use for the temperature submissions.

**Reference**

[1] Hankins H. *Stand-alone solar electric systems*. London: Earthscan; 2010.

[2] Wong J, Sridharan R, Shanmugam V. *Quantifying edge and peripheral recombination losses in industrial silicon solar cells*. IEEE Trans Electron Devices 2015;62(11):3750–5. Article No.7289429.

[3] H.M. Ali, M. Mahmood, M.A. Bashir, M. Ali, A.M. Siddiqui, *Outdoor testing of photovoltaic modules during summer in Taxila*, Pakistan, J. Therm. Sci. (2013).

[4] Reddy, S.R., Ebadian, M.A., Lin, C.-X., 2015. *A review of PV–T systems: thermal management and efficiency with single-phase cooling*. Int. J. Heat Mass Transf. 91, 861–871.

[5] Koehl, M., Heck, M., Wiesmeier, S., Wirth, J., 2012. *Modelling of conditions for accelerated lifetime testing of Humidity impact on PV-modules based on monitoring of climatic data*. Sol. Energy Mater. Sol. Cells 99, 282–291.

[6] Zhu L, Raman AP, Fan S. *Radiative cooling of solar absorbers using a visibly transparent photonic crystal thermal blackbody*. Proc Natl AcadSci 2015;112 (40):12282–7.

[7] Debra H. *An investigation on energy performance assessment of a photovoltaic solar wall under buoyancy-induced and fan-assisted ventilation system*. Appl Energy 2017; 191: 55–74.

[8] Luque A, Sala G, Arboiro JC. *Electric and thermal model for non-uniformly illuminated concentration cells*. Sol Energy Mater Sol Cells 1998;51(3– 4):269–90.

[9] Royne A, Dey C, Mills D. *Cooling of photovoltaic cells under concentrated illumination: a critical review*. Sol Energy Mater Sol Cells 2005;86(4):451– 83.

[10] Cynthia Christabel S, Srinivasan A and Prince Winston D,(2016) “*Couple Matching Best Generation Algorithm for Partially Shaded Photovoltaic Systems*,” Journal of Electrical Engineering, vol. 16, no. 3, pp. 382-391, 2016.

[11] Praveen Kumar B, Prince Winston D, Cynthia Christabel S, et al. (2017), ‘[*Implementation of a Switched PV Technique for Rooftop 2 kW Solar PV to Enhance Power during Unavoidable Partial Shading Conditions*](https://www.researchgate.net/profile/Praveen_b/publication/321161756_Implementation_of_a_Switched_PV_Technique_for_Rooftop_2_kW_Solar_PV_to_Enhance_Power_during_Unavoidable_Partial_Shading_Conditions/links/5a1293cf0f7e9bd1b2c11489/Implementation-of-a-Switched-PV-Technique-for-Rooftop-2-kW-Solar-PV-to-Enhance-Power-during-Unavoidable-Partial-Shading-Conditions.pdf)’ Journal of Power Electronics, 17 (6), 1600-1610. DOI: 10.6113/JPE.2017.17.6.1600.

[12] Prince Winston D, Praveen Kumar B, Cynthia Christabel S (2018) “*Maximum power extraction in solar renewable power system - a bypass diode scanning approach*,” Computers and Electrical Engineering 2018, 70, pp. 122-136.

[13] D. Prince Winston,S. Kumaravel, B. Praveen Kumar, S. Devakirubakaran (2019) “*Performance improvement of solar PV array topologies during various partial shading conditions*” Solar Energy-Elsevier (196), pp.228–242.

[14] Edenburn MW, Burns JR. *Shading analysis of a photovoltaic-cell string illuminated by a parabolic-trough concentrator. NASA STI/Recon Technical Report* N, vol. 83; Sep. 1982. p. 21537.

[15] Benemann J, Chehab O, Schaar-Gabriel E. *Building-integrated PV modules*. Sol Energy Mater Sol Cells 2001;67:345–54.

[16] Bazilian M, Leenders F, Van Der Ree BGC, *Prasad D. Photovoltaic cogeneration in the built environment*. Sol Energy 2001;71:57–69.

[17] Naphon P. *On the performance and entropy generation of the double-pass solar air heater with longitudinal fins*. Renew Energy 2005;30:1345–57.

[18] Kolb A, Winter ERF, Viskanta R. *Experimental studies on a solar air collector with metal matrix absorber*. Sol Energy 1999;65:91–8.

[19] Choudhury C, Garg HP. *Performance of air-heating collector with packed airflow passage*. Sol Energy 1993;50:205–21.

[20] Krauter S. *Increased electrical yield via water flow over the front of photovoltaic panels*. Solar Energy Materials & Solar Cells 2004;82:131e7.

[21] Saad O, Masud B. *Improving photovoltaic module efficiency using water cooling*. Heat Transfer Engineering 2009;30(6):499e505.

[22] Abdolzadeh M, Ameri M. *Improving the effectiveness of a PV water pumping system by spraying water over the front of photovoltaic cells*. Renewable Energy 2009;34:91e6.

[23] Rosa CM, Rosa CP, Tina GM, Scandura PF. *Submerged photovoltaic solar panel: SP2*. Renewable Energy 2010;35(8):1862e5.

[24] Prakash, J., 1994. *Transient analysis of a photovoltaic/thermal solar collector for co-generation of electricity and hot air/water.* Energy Conversion and Management 35, 967–972.

[25] Oommen TV. *Vegetable oils for liquid-filled transformers*. IEEE ElectrInsul  
Mag 2002;18 (1):7–11.

[26] F. Qiu, et al., *Biodiesel production from mixed soybean oil and rapeseed oil*, Appl. Energy 88 (2011) 2050–2055.

[27] Shahidi F, editor. *6th edition Bailey's Industrial oil and fat products*, 1–6. Hoboken, New Jersey: Published by John Wiley & Sons, Inc.; 2005.

[28] SabarinathSankaran Nair, KumarapillaiPrabhakaran Nair and Perikinalil Krishnan Rajendrakumar “*Evaluation of physicochemical, thermal and tribological properties of sesame oil (Sesamumindicum L.): a potential agricultural crop base stock for eco-friendly industrial lubricants*, Int. J. Agricultural Resources, Governance and Ecology, Vol. 13, No. 1, 2017.